

ScanPrint scanner firmware update


* Plug in the USB lead.
* Run HSC\_PROG.exe
* The window should display Vendor ID, Product ID, Product Version and other information.



* Click the "Prog Fw" button



* The window should display "Erasing SPI Flash"
* The final message should be "FPGA Programming in SPI flash Done".



* Exit the program