ScanPrint scanner firmware update

* Plug in the USB lead.
* Run HSC\_PROG.exe
* The window should display Vendor ID, Product ID, Product Version and other information.

* Click the "Prog Fw" button

* The window should display "Erasing SPI Flash"
* The final message should be "FPGA Programming in SPI flash Done".

* Exit the program